ARM CPU Specific Build Macros
=============================

Contents
--------

1.  [Introduction](#1--introduction)
2.  [CPU Errata Workarounds](#2--cpu-errata-workarounds)
3.  [CPU Specific optimizations](#3--cpu-specific-optimizations)


1.  Introduction
----------------

This document describes the various build options present in the CPU specific
operations framework to enable errata workarounds and to enable optimizations
for a specific CPU on a platform.

2.  CPU Errata Workarounds
--------------------------

ARM Trusted Firmware exports a series of build flags which control the
errata workarounds that are applied to each CPU by the reset handler. The
errata details can be found in the CPU specific errata documents published
by ARM:

*   [Cortex-A53 MPCore Software Developers Errata Notice][A53 Errata Notice]
*   [Cortex-A57 MPCore Software Developers Errata Notice][A57 Errata Notice]

The errata workarounds are implemented for a particular revision or a set of
processor revisions. This is checked by the reset handler at runtime. Each
errata workaround is identified by its `ID` as specified in the processor's
errata notice document. The format of the define used to enable/disable the
errata workaround is `ERRATA_<Processor name>_<ID>`, where the `Processor name`
is for example `A57` for the `Cortex_A57` CPU.

Refer to the section _CPU errata status reporting_ in [Firmware Design
guide][Firmware Design] for information on to write errata workaround functions.

All workarounds are disabled by default. The platform is responsible for
enabling these workarounds according to its requirement by defining the
errata workaround build flags in the platform specific makefile. In case
these workarounds are enabled for the wrong CPU revision then the errata
workaround is not applied. In the DEBUG build, this is indicated by
printing a warning to the crash console.

In the current implementation, a platform which has more than 1 variant
with different revisions of a processor has no runtime mechanism available
for it to specify which errata workarounds should be enabled or not.

The value of the build flags are 0 by default, that is, disabled. Any other
value will enable it.

For Cortex-A53, following errata build flags are defined :

*   `ERRATA_A53_826319`: This applies errata 826319 workaround to Cortex-A53
     CPU. This needs to be enabled only for revision <= r0p2 of the CPU.

*   `ERRATA_A53_836870`: This applies errata 836870 workaround to Cortex-A53
     CPU. This needs to be enabled only for revision <= r0p3 of the CPU. From
     r0p4 and onwards, this errata is enabled by default.

For Cortex-A57, following errata build flags are defined :

*   `ERRATA_A57_806969`: This applies errata 806969 workaround to Cortex-A57
     CPU. This needs to be enabled only for revision r0p0 of the CPU.

*   `ERRATA_A57_813420`: This applies errata 813420 workaround to Cortex-A57
     CPU. This needs to be enabled only for revision r0p0 of the CPU.

*   `ERRATA_A57_826974`: This applies errata 826974 workaround to Cortex-A57
     CPU. This needs to be enabled only for revision <= r1p1 of the CPU.

*   `ERRATA_A57_826977`: This applies errata 826977 workaround to Cortex-A57
     CPU. This needs to be enabled only for revision <= r1p1 of the CPU.

*   `ERRATA_A57_828024`: This applies errata 828024 workaround to Cortex-A57
     CPU. This needs to be enabled only for revision <= r1p1 of the CPU.

*   `ERRATA_A57_829520`: This applies errata 829520 workaround to Cortex-A57
     CPU. This needs to be enabled only for revision <= r1p2 of the CPU.

*   `ERRATA_A57_833471`: This applies errata 833471 workaround to Cortex-A57
     CPU. This needs to be enabled only for revision <= r1p2 of the CPU.

3.  CPU Specific optimizations
------------------------------

This section describes some of the optimizations allowed by the CPU micro
architecture that can be enabled by the platform as desired.

*    `SKIP_A57_L1_FLUSH_PWR_DWN`: This flag enables an optimization in the
     Cortex-A57 cluster power down sequence by not flushing the Level 1 data
     cache. The L1 data cache and the L2 unified cache are inclusive. A flush
     of the L2 by set/way flushes any dirty lines from the L1 as well. This
     is a known safe deviation from the Cortex-A57 TRM defined power down
     sequence. Each Cortex-A57 based platform must make its own decision on
     whether to use the optimization.

*    `A53_DISABLE_NON_TEMPORAL_HINT`: This flag disables the cache non-temporal
     hint. The LDNP/STNP instructions as implemented on Cortex-A53 do not behave
     in a way most programmers expect, and will most probably result in a
     significant speed degradation to any code that employs them. The ARMv8-A
     architecture (see ARM DDI 0487A.h, section D3.4.3) allows cores to ignore
     the non-temporal hint and treat LDNP/STNP as LDP/STP instead. Enabling this
     flag enforces this behaviour. This needs to be enabled only for revisions
     <= r0p3 of the CPU and is enabled by default.

*    `A57_DISABLE_NON_TEMPORAL_HINT`: This flag has the same behaviour as
     `A53_DISABLE_NON_TEMPORAL_HINT` but for Cortex-A57. This needs to be
     enabled only for revisions <= r1p2 of the CPU and is enabled by default,
     as recommended in section "4.7 Non-Temporal Loads/Stores" of the
     [Cortex-A57 Software Optimization Guide][A57 SW Optimization Guide].

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

_Copyright (c) 2014-2016, ARM Limited and Contributors. All rights reserved._

[A57 SW Optimization Guide]: http://infocenter.arm.com/help/topic/com.arm.doc.uan0015b/Cortex_A57_Software_Optimization_Guide_external.pdf
[A53 Errata Notice]:         http://infocenter.arm.com/help/topic/com.arm.doc.epm048406/index.html
[A57 Errata Notice]:         http://infocenter.arm.com/help/topic/com.arm.doc.epm049219/cortex_a57_mpcore_software_developers_errata_notice.pdf
[Firmware Design]:           firmware-design.md
