/*
 * Copyright (c) 2019, Arm Limited. All rights reserved.
 *
 * SPDX-License-Identifier: BSD-3-Clause
 */

/dts-v1/;

/ {
	model = "A5DS";
	compatible = "arm,A5DS";
	interrupt-parent = <&gic>;
	#address-cells = <1>;
	#size-cells = <1>;

	psci {
		compatible = "arm,psci-1.0", "arm,psci-0.2", "arm,psci";
		method = "smc";
		cpu_on = <0x84000003>;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;
		cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a5";
			enable-method = "psci";
			reg = <0>;
		};
		cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a5";
			enable-method = "psci";
			reg = <1>;
		};
		cpu@2 {
			device_type = "cpu";
			compatible = "arm,cortex-a5";
			enable-method = "psci";
			reg = <2>;
		};
		cpu@3 {
			device_type = "cpu";
			compatible = "arm,cortex-a5";
			enable-method = "psci";
			reg = <3>;
		};
	};

	memory@80000000 {
		device_type = "memory";
		reg = <0x80000000 0x7F000000>;
	};

	refclk100mhz: refclk100mhz {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <100000000>;
		clock-output-names = "apb_pclk";
	};

	smbclk: refclk24mhzx2 {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <48000000>;
		clock-output-names = "smclk";
	};


	rtc@1a220000 {
		compatible = "arm,pl031", "arm,primecell";
		reg = <0x1a220000 0x1000>;
		clocks = <&refclk100mhz>;
		interrupts = <0 6 0xf04>;
		clock-names = "apb_pclk";
	};

	gic: interrupt-controller@1c001000 {
		compatible = "arm,cortex-a9-gic";
		#interrupt-cells = <3>;
		#address-cells = <0>;
		interrupt-controller;
		reg = <0x1c001000 0x1000>,
			  <0x1c000100 0x100>;
		interrupts = <1 9 0xf04>;
	};

	serial0: uart@1a200000 {
		compatible = "arm,pl011", "arm,primecell";
		reg = <0x1a200000 0x1000>;
		interrupt-parent = <&gic>;
		interrupts = <0 8 0xf04>;
		clocks = <&refclk100mhz>;
		clock-names = "apb_pclk";
	};

	serial1: uart@1a210000 {
		compatible = "arm,pl011", "arm,primecell";
		reg = <0x1a210000 0x1000>;
		interrupt-parent = <&gic>;
		interrupts = <0 9 0xf04>;
		clocks = <&refclk100mhz>;
		clock-names = "apb_pclk";
	};

	timer0: timer@1a040000 {
		compatible = "arm,armv7-timer-mem";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		reg = <0x1a040000 0x1000>;
		clock-frequency = <50000000>;

		frame@1a050000 {
			frame-number = <0>;
			interrupts = <0 2 0xf04>;
			reg = <0x1a050000 0x1000>;
		};
	};
};
