/*
 * Copyright (c) 2013-2020, ARM Limited and Contributors. All rights reserved.
 *
 * SPDX-License-Identifier: BSD-3-Clause
 */

/* Configuration: 1 cluster with up to 4 CPUs */

/dts-v1/;

#define	AFF
#define	CLUSTER_COUNT	1

#include "fvp-defs.dtsi"

/memreserve/ 0x80000000 0x00010000;

/ {
};

/ {
	model = "FVP Foundation";
	compatible = "arm,fvp-base", "arm,vexpress";
	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	chosen { };

	aliases {
		serial0 = &v2m_serial0;
		serial1 = &v2m_serial1;
		serial2 = &v2m_serial2;
		serial3 = &v2m_serial3;
	};

	psci {
		compatible = "arm,psci-1.0", "arm,psci-0.2", "arm,psci";
		method = "smc";
		cpu_suspend = <0xc4000001>;
		cpu_off = <0x84000002>;
		cpu_on = <0xc4000003>;
		sys_poweroff = <0x84000008>;
		sys_reset = <0x84000009>;
		max-pwr-lvl = <2>;
	};

	cpus {
		#address-cells = <2>;
		#size-cells = <0>;

		CPU_MAP

		idle-states {
			entry-method = "arm,psci";

			CPU_SLEEP_0: cpu-sleep-0 {
				compatible = "arm,idle-state";
				local-timer-stop;
				arm,psci-suspend-param = <0x0010000>;
				entry-latency-us = <40>;
				exit-latency-us = <100>;
				min-residency-us = <150>;
			};

			CLUSTER_SLEEP_0: cluster-sleep-0 {
				compatible = "arm,idle-state";
				local-timer-stop;
				arm,psci-suspend-param = <0x1010000>;
				entry-latency-us = <500>;
				exit-latency-us = <1000>;
				min-residency-us = <2500>;
			};
		};

		CPUS

		L2_0: l2-cache0 {
			compatible = "cache";
		};
	};

	memory@80000000 {
		device_type = "memory";
		reg = <0x00000000 0x80000000 0 0x7F000000>,
		      <0x00000008 0x80000000 0 0x80000000>;
	};

	gic: interrupt-controller@2f000000 {
		compatible = "arm,cortex-a15-gic", "arm,cortex-a9-gic";
		#interrupt-cells = <3>;
		#address-cells = <0>;
		interrupt-controller;
		reg = <0x0 0x2f000000 0 0x10000>,
		      <0x0 0x2c000000 0 0x2000>,
		      <0x0 0x2c010000 0 0x2000>,
		      <0x0 0x2c02F000 0 0x2000>;
		interrupts = <1 9 0xf04>;
	};

	timer {
		compatible = "arm,armv8-timer";
		interrupts = <1 13 0xff01>,
			     <1 14 0xff01>,
			     <1 11 0xff01>,
			     <1 10 0xff01>;
		clock-frequency = <100000000>;
	};

	timer@2a810000 {
			compatible = "arm,armv7-timer-mem";
			reg = <0x0 0x2a810000 0x0 0x10000>;
			clock-frequency = <100000000>;
			#address-cells = <2>;
			#size-cells = <2>;
			ranges;
			frame@2a830000 {
				frame-number = <1>;
				interrupts = <0 26 4>;
				reg = <0x0 0x2a830000 0x0 0x10000>;
			};
	};

	pmu {
		compatible = "arm,armv8-pmuv3";
		interrupts = <0 60 4>,
			     <0 61 4>,
			     <0 62 4>,
			     <0 63 4>;
	};

	smb {
		compatible = "simple-bus";

		#address-cells = <2>;
		#size-cells = <1>;
		ranges = <0 0 0 0x08000000 0x04000000>,
			 <1 0 0 0x14000000 0x04000000>,
			 <2 0 0 0x18000000 0x04000000>,
			 <3 0 0 0x1c000000 0x04000000>,
			 <4 0 0 0x0c000000 0x04000000>,
			 <5 0 0 0x10000000 0x04000000>;

		#include "fvp-foundation-motherboard.dtsi"
	};
};
