Build Options
=============

The TF-A build system supports the following build options. Unless mentioned
otherwise, these options are expected to be specified at the build command
line and are not to be modified in any component makefiles. Note that the
build system doesn't track dependency for build options. Therefore, if any of
the build options are changed from a previous build, a clean build must be
performed.

.. _build_options_common:

Common build options
--------------------

-  ``AARCH32_INSTRUCTION_SET``: Choose the AArch32 instruction set that the
   compiler should use. Valid values are T32 and A32. It defaults to T32 due to
   code having a smaller resulting size.

-  ``AARCH32_SP`` : Choose the AArch32 Secure Payload component to be built as
   as the BL32 image when ``ARCH=aarch32``. The value should be the path to the
   directory containing the SP source, relative to the ``bl32/``; the directory
   is expected to contain a makefile called ``<aarch32_sp-value>.mk``.

-  ``AMU_RESTRICT_COUNTERS``: Register reads to the group 1 counters will return
   zero at all but the highest implemented exception level.  Reads from the
   memory mapped view are unaffected by this control.

-  ``ARCH`` : Choose the target build architecture for TF-A. It can take either
   ``aarch64`` or ``aarch32`` as values. By default, it is defined to
   ``aarch64``.

-  ``ARM_ARCH_FEATURE``: Optional Arm Architecture build option which specifies
   one or more feature modifiers. This option has the form ``[no]feature+...``
   and defaults to ``none``. It translates into compiler option
   ``-march=armvX[.Y]-a+[no]feature+...``. See compiler's documentation for the
   list of supported feature modifiers.

-  ``ARM_ARCH_MAJOR``: The major version of Arm Architecture to target when
   compiling TF-A. Its value must be numeric, and defaults to 8 . See also,
   *Armv8 Architecture Extensions* and *Armv7 Architecture Extensions* in
   :ref:`Firmware Design`.

-  ``ARM_ARCH_MINOR``: The minor version of Arm Architecture to target when
   compiling TF-A. Its value must be a numeric, and defaults to 0. See also,
   *Armv8 Architecture Extensions* in :ref:`Firmware Design`.

-  ``BL2``: This is an optional build option which specifies the path to BL2
   image for the ``fip`` target. In this case, the BL2 in the TF-A will not be
   built.

-  ``BL2U``: This is an optional build option which specifies the path to
   BL2U image. In this case, the BL2U in TF-A will not be built.

-  ``BL2_AT_EL3``: This is an optional build option that enables the use of
   BL2 at EL3 execution level.

-  ``BL2_IN_XIP_MEM``: In some use-cases BL2 will be stored in eXecute In Place
   (XIP) memory, like BL1. In these use-cases, it is necessary to initialize
   the RW sections in RAM, while leaving the RO sections in place. This option
   enable this use-case. For now, this option is only supported when BL2_AT_EL3
   is set to '1'.

-  ``BL31``: This is an optional build option which specifies the path to
   BL31 image for the ``fip`` target. In this case, the BL31 in TF-A will not
   be built.

-  ``BL31_KEY``: This option is used when ``GENERATE_COT=1``. It specifies the
   file that contains the BL31 private key in PEM format. If ``SAVE_KEYS=1``,
   this file name will be used to save the key.

-  ``BL32``: This is an optional build option which specifies the path to
   BL32 image for the ``fip`` target. In this case, the BL32 in TF-A will not
   be built.

-  ``BL32_EXTRA1``: This is an optional build option which specifies the path to
   Trusted OS Extra1 image for the  ``fip`` target.

-  ``BL32_EXTRA2``: This is an optional build option which specifies the path to
   Trusted OS Extra2 image for the ``fip`` target.

-  ``BL32_KEY``: This option is used when ``GENERATE_COT=1``. It specifies the
   file that contains the BL32 private key in PEM format. If ``SAVE_KEYS=1``,
   this file name will be used to save the key.

-  ``BL33``: Path to BL33 image in the host file system. This is mandatory for
   ``fip`` target in case TF-A BL2 is used.

-  ``BL33_KEY``: This option is used when ``GENERATE_COT=1``. It specifies the
   file that contains the BL33 private key in PEM format. If ``SAVE_KEYS=1``,
   this file name will be used to save the key.

-  ``BRANCH_PROTECTION``: Numeric value to enable ARMv8.3 Pointer Authentication
   and ARMv8.5 Branch Target Identification support for TF-A BL images themselves.
   If enabled, it is needed to use a compiler that supports the option
   ``-mbranch-protection``. Selects the branch protection features to use:
-  0: Default value turns off all types of branch protection
-  1: Enables all types of branch protection features
-  2: Return address signing to its standard level
-  3: Extend the signing to include leaf functions
-  4: Turn on branch target identification mechanism

   The table below summarizes ``BRANCH_PROTECTION`` values, GCC compilation options
   and resulting PAuth/BTI features.

   +-------+--------------+-------+-----+
   | Value |  GCC option  | PAuth | BTI |
   +=======+==============+=======+=====+
   |   0   |     none     |   N   |  N  |
   +-------+--------------+-------+-----+
   |   1   |   standard   |   Y   |  Y  |
   +-------+--------------+-------+-----+
   |   2   |   pac-ret    |   Y   |  N  |
   +-------+--------------+-------+-----+
   |   3   | pac-ret+leaf |   Y   |  N  |
   +-------+--------------+-------+-----+
   |   4   |     bti      |   N   |  Y  |
   +-------+--------------+-------+-----+

   This option defaults to 0 and this is an experimental feature.
   Note that Pointer Authentication is enabled for Non-secure world
   irrespective of the value of this option if the CPU supports it.

-  ``BUILD_MESSAGE_TIMESTAMP``: String used to identify the time and date of the
   compilation of each build. It must be set to a C string (including quotes
   where applicable). Defaults to a string that contains the time and date of
   the compilation.

-  ``BUILD_STRING``: Input string for VERSION_STRING, which allows the TF-A
   build to be uniquely identified. Defaults to the current git commit id.

-  ``BUILD_BASE``: Output directory for the build. Defaults to ``./build``

-  ``CFLAGS``: Extra user options appended on the compiler's command line in
   addition to the options set by the build system.

-  ``COLD_BOOT_SINGLE_CPU``: This option indicates whether the platform may
   release several CPUs out of reset. It can take either 0 (several CPUs may be
   brought up) or 1 (only one CPU will ever be brought up during cold reset).
   Default is 0. If the platform always brings up a single CPU, there is no
   need to distinguish between primary and secondary CPUs and the boot path can
   be optimised. The ``plat_is_my_cpu_primary()`` and
   ``plat_secondary_cold_boot_setup()`` platform porting interfaces do not need
   to be implemented in this case.

-  ``COT``: When Trusted Boot is enabled, selects the desired chain of trust.
   Defaults to ``tbbr``.

-  ``CRASH_REPORTING``: A non-zero value enables a console dump of processor
   register state when an unexpected exception occurs during execution of
   BL31. This option defaults to the value of ``DEBUG`` - i.e. by default
   this is only enabled for a debug build of the firmware.

-  ``CREATE_KEYS``: This option is used when ``GENERATE_COT=1``. It tells the
   certificate generation tool to create new keys in case no valid keys are
   present or specified. Allowed options are '0' or '1'. Default is '1'.

-  ``CTX_INCLUDE_AARCH32_REGS`` : Boolean option that, when set to 1, will cause
   the AArch32 system registers to be included when saving and restoring the
   CPU context. The option must be set to 0 for AArch64-only platforms (that
   is on hardware that does not implement AArch32, or at least not at EL1 and
   higher ELs). Default value is 1.

-  ``CTX_INCLUDE_EL2_REGS`` : This boolean option provides context save/restore
   operations when entering/exiting an EL2 execution context. This is of primary
   interest when Armv8.4-SecEL2 extension is implemented. Default is 0 (disabled).
   This option must be equal to 1 (enabled) when ``SPD=spmd`` and
   ``SPMD_SPM_AT_SEL2`` is set.

-  ``CTX_INCLUDE_FPREGS``: Boolean option that, when set to 1, will cause the FP
   registers to be included when saving and restoring the CPU context. Default
   is 0.

-  ``CTX_INCLUDE_NEVE_REGS``: Boolean option that, when set to 1, will cause the
   Armv8.4-NV registers to be saved/restored when entering/exiting an EL2
   execution context. Default value is 0.

-  ``CTX_INCLUDE_PAUTH_REGS``: Boolean option that, when set to 1, enables
   Pointer Authentication for Secure world. This will cause the ARMv8.3-PAuth
   registers to be included when saving and restoring the CPU context as
   part of world switch. Default value is 0 and this is an experimental feature.
   Note that Pointer Authentication is enabled for Non-secure world irrespective
   of the value of this flag if the CPU supports it.

-  ``DEBUG``: Chooses between a debug and release build. It can take either 0
   (release) or 1 (debug) as values. 0 is the default.

-  ``DECRYPTION_SUPPORT``: This build flag enables the user to select the
   authenticated decryption algorithm to be used to decrypt firmware/s during
   boot. It accepts 2 values: ``aes_gcm`` and ``none``. The default value of
   this flag is ``none`` to disable firmware decryption which is an optional
   feature as per TBBR. Also, it is an experimental feature.

-  ``DISABLE_BIN_GENERATION``: Boolean option to disable the generation
   of the binary image. If set to 1, then only the ELF image is built.
   0 is the default.

-  ``DISABLE_MTPMU``: Boolean option to disable FEAT_MTPMU if implemented
   (Armv8.6 onwards). Its default value is 0 to keep consistency with platforms
   that do not implement FEAT_MTPMU. For more information on FEAT_MTPMU,
   check the latest Arm ARM.

-  ``DYN_DISABLE_AUTH``: Provides the capability to dynamically disable Trusted
   Board Boot authentication at runtime. This option is meant to be enabled only
   for development platforms. ``TRUSTED_BOARD_BOOT`` flag must be set if this
   flag has to be enabled. 0 is the default.

-  ``E``: Boolean option to make warnings into errors. Default is 1.

-  ``EL3_PAYLOAD_BASE``: This option enables booting an EL3 payload instead of
   the normal boot flow. It must specify the entry point address of the EL3
   payload. Please refer to the "Booting an EL3 payload" section for more
   details.

-  ``ENABLE_AMU``: Boolean option to enable Activity Monitor Unit extensions.
   This is an optional architectural feature available on v8.4 onwards. Some
   v8.2 implementations also implement an AMU and this option can be used to
   enable this feature on those systems as well. Default is 0.

-  ``ENABLE_ASSERTIONS``: This option controls whether or not calls to ``assert()``
   are compiled out. For debug builds, this option defaults to 1, and calls to
   ``assert()`` are left in place. For release builds, this option defaults to 0
   and calls to ``assert()`` function are compiled out. This option can be set
   independently of ``DEBUG``. It can also be used to hide any auxiliary code
   that is only required for the assertion and does not fit in the assertion
   itself.

-  ``ENABLE_BACKTRACE``: This option controls whether to enable backtrace
   dumps or not. It is supported in both AArch64 and AArch32. However, in
   AArch32 the format of the frame records are not defined in the AAPCS and they
   are defined by the implementation. This implementation of backtrace only
   supports the format used by GCC when T32 interworking is disabled. For this
   reason enabling this option in AArch32 will force the compiler to only
   generate A32 code. This option is enabled by default only in AArch64 debug
   builds, but this behaviour can be overridden in each platform's Makefile or
   in the build command line.

-  ``ENABLE_LTO``: Boolean option to enable Link Time Optimization (LTO)
   support in GCC for TF-A. This option is currently only supported for
   AArch64. Default is 0.

-  ``ENABLE_MPAM_FOR_LOWER_ELS``: Boolean option to enable lower ELs to use MPAM
   feature. MPAM is an optional Armv8.4 extension that enables various memory
   system components and resources to define partitions; software running at
   various ELs can assign themselves to desired partition to control their
   performance aspects.

   When this option is set to ``1``, EL3 allows lower ELs to access their own
   MPAM registers without trapping into EL3. This option doesn't make use of
   partitioning in EL3, however. Platform initialisation code should configure
   and use partitions in EL3 as required. This option defaults to ``0``.

-  ``ENABLE_PIE``: Boolean option to enable Position Independent Executable(PIE)
   support within generic code in TF-A. This option is currently only supported
   in BL2_AT_EL3, BL31, and BL32 (TSP) for AARCH64 binaries, and in BL32
   (SP_min) for AARCH32. Default is 0.

-  ``ENABLE_PMF``: Boolean option to enable support for optional Performance
   Measurement Framework(PMF). Default is 0.

-  ``ENABLE_PSCI_STAT``: Boolean option to enable support for optional PSCI
   functions ``PSCI_STAT_RESIDENCY`` and ``PSCI_STAT_COUNT``. Default is 0.
   In the absence of an alternate stat collection backend, ``ENABLE_PMF`` must
   be enabled. If ``ENABLE_PMF`` is set, the residency statistics are tracked in
   software.

-  ``ENABLE_RUNTIME_INSTRUMENTATION``: Boolean option to enable runtime
   instrumentation which injects timestamp collection points into TF-A to
   allow runtime performance to be measured. Currently, only PSCI is
   instrumented. Enabling this option enables the ``ENABLE_PMF`` build option
   as well. Default is 0.

-  ``ENABLE_SPE_FOR_LOWER_ELS`` : Boolean option to enable Statistical Profiling
   extensions. This is an optional architectural feature for AArch64.
   The default is 1 but is automatically disabled when the target architecture
   is AArch32.

-  ``ENABLE_SVE_FOR_NS``: Boolean option to enable Scalable Vector Extension
   (SVE) for the Non-secure world only. SVE is an optional architectural feature
   for AArch64. Note that when SVE is enabled for the Non-secure world, access
   to SIMD and floating-point functionality from the Secure world is disabled by
   default and controlled with ENABLE_SVE_FOR_SWD.
   This is to avoid corruption of the Non-secure world data in the Z-registers
   which are aliased by the SIMD and FP registers. The build option is not
   compatible with the ``CTX_INCLUDE_FPREGS`` build option, and will raise an
   assert on platforms where SVE is implemented and ``ENABLE_SVE_FOR_NS`` set to
   1. The default is 1 but is automatically disabled when the target
   architecture is AArch32.

-  ``ENABLE_SVE_FOR_SWD``: Boolean option to enable SVE for the Secure world.
   SVE is an optional architectural feature for AArch64. Note that this option
   requires ENABLE_SVE_FOR_NS to be enabled.  The default is 0 and it is
   automatically disabled when the target architecture is AArch32.

-  ``ENABLE_STACK_PROTECTOR``: String option to enable the stack protection
   checks in GCC. Allowed values are "all", "strong", "default" and "none". The
   default value is set to "none". "strong" is the recommended stack protection
   level if this feature is desired. "none" disables the stack protection. For
   all values other than "none", the ``plat_get_stack_protector_canary()``
   platform hook needs to be implemented. The value is passed as the last
   component of the option ``-fstack-protector-$ENABLE_STACK_PROTECTOR``.

-  ``ENCRYPT_BL31``: Binary flag to enable encryption of BL31 firmware. This
   flag depends on ``DECRYPTION_SUPPORT`` build flag which is marked as
   experimental.

-  ``ENCRYPT_BL32``: Binary flag to enable encryption of Secure BL32 payload.
   This flag depends on ``DECRYPTION_SUPPORT`` build flag which is marked as
   experimental.

-  ``ENC_KEY``: A 32-byte (256-bit) symmetric key in hex string format. It could
   either be SSK or BSSK depending on ``FW_ENC_STATUS`` flag. This value depends
   on ``DECRYPTION_SUPPORT`` build flag which is marked as experimental.

-  ``ENC_NONCE``: A 12-byte (96-bit) encryption nonce or Initialization Vector
   (IV) in hex string format. This value depends on ``DECRYPTION_SUPPORT``
   build flag which is marked as experimental.

-  ``ERROR_DEPRECATED``: This option decides whether to treat the usage of
   deprecated platform APIs, helper functions or drivers within Trusted
   Firmware as error. It can take the value 1 (flag the use of deprecated
   APIs as error) or 0. The default is 0.

-  ``EL3_EXCEPTION_HANDLING``: When set to ``1``, enable handling of exceptions
   targeted at EL3. When set ``0`` (default), no exceptions are expected or
   handled at EL3, and a panic will result. This is supported only for AArch64
   builds.

-  ``EVENT_LOG_LEVEL``: Chooses the log level to use for Measured Boot when
   ``MEASURED_BOOT`` is enabled. For a list of valid values, see ``LOG_LEVEL``.
   Default value is 40 (LOG_LEVEL_INFO).

-  ``FAULT_INJECTION_SUPPORT``: ARMv8.4 extensions introduced support for fault
   injection from lower ELs, and this build option enables lower ELs to use
   Error Records accessed via System Registers to inject faults. This is
   applicable only to AArch64 builds.

   This feature is intended for testing purposes only, and is advisable to keep
   disabled for production images.

-  ``FIP_NAME``: This is an optional build option which specifies the FIP
   filename for the ``fip`` target. Default is ``fip.bin``.

-  ``FWU_FIP_NAME``: This is an optional build option which specifies the FWU
   FIP filename for the ``fwu_fip`` target. Default is ``fwu_fip.bin``.

-  ``FW_ENC_STATUS``: Top level firmware's encryption numeric flag, values:

   ::

     0: Encryption is done with Secret Symmetric Key (SSK) which is common
        for a class of devices.
     1: Encryption is done with Binding Secret Symmetric Key (BSSK) which is
        unique per device.

   This flag depends on ``DECRYPTION_SUPPORT`` build flag which is marked as
   experimental.

-  ``GENERATE_COT``: Boolean flag used to build and execute the ``cert_create``
   tool to create certificates as per the Chain of Trust described in
   :ref:`Trusted Board Boot`. The build system then calls ``fiptool`` to
   include the certificates in the FIP and FWU_FIP. Default value is '0'.

   Specify both ``TRUSTED_BOARD_BOOT=1`` and ``GENERATE_COT=1`` to include support
   for the Trusted Board Boot feature in the BL1 and BL2 images, to generate
   the corresponding certificates, and to include those certificates in the
   FIP and FWU_FIP.

   Note that if ``TRUSTED_BOARD_BOOT=0`` and ``GENERATE_COT=1``, the BL1 and BL2
   images will not include support for Trusted Board Boot. The FIP will still
   include the corresponding certificates. This FIP can be used to verify the
   Chain of Trust on the host machine through other mechanisms.

   Note that if ``TRUSTED_BOARD_BOOT=1`` and ``GENERATE_COT=0``, the BL1 and BL2
   images will include support for Trusted Board Boot, but the FIP and FWU_FIP
   will not include the corresponding certificates, causing a boot failure.

-  ``GICV2_G0_FOR_EL3``: Unlike GICv3, the GICv2 architecture doesn't have
   inherent support for specific EL3 type interrupts. Setting this build option
   to ``1`` assumes GICv2 *Group 0* interrupts are expected to target EL3, both
   by :ref:`platform abstraction layer<platform Interrupt Controller API>` and
   :ref:`Interrupt Management Framework<Interrupt Management Framework>`.
   This allows GICv2 platforms to enable features requiring EL3 interrupt type.
   This also means that all GICv2 Group 0 interrupts are delivered to EL3, and
   the Secure Payload interrupts needs to be synchronously handed over to Secure
   EL1 for handling. The default value of this option is ``0``, which means the
   Group 0 interrupts are assumed to be handled by Secure EL1.

-  ``HANDLE_EA_EL3_FIRST``: When set to ``1``, External Aborts and SError
   Interrupts will be always trapped in EL3 i.e. in BL31 at runtime. When set to
   ``0`` (default), these exceptions will be trapped in the current exception
   level (or in EL1 if the current exception level is EL0).

-  ``HW_ASSISTED_COHERENCY``: On most Arm systems to-date, platform-specific
   software operations are required for CPUs to enter and exit coherency.
   However, newer systems exist where CPUs' entry to and exit from coherency
   is managed in hardware. Such systems require software to only initiate these
   operations, and the rest is managed in hardware, minimizing active software
   management. In such systems, this boolean option enables TF-A to carry out
   build and run-time optimizations during boot and power management operations.
   This option defaults to 0 and if it is enabled, then it implies
   ``WARMBOOT_ENABLE_DCACHE_EARLY`` is also enabled.

   If this flag is disabled while the platform which TF-A is compiled for
   includes cores that manage coherency in hardware, then a compilation error is
   generated. This is based on the fact that a system cannot have, at the same
   time, cores that manage coherency in hardware and cores that don't. In other
   words, a platform cannot have, at the same time, cores that require
   ``HW_ASSISTED_COHERENCY=1`` and cores that require
   ``HW_ASSISTED_COHERENCY=0``.

   Note that, when ``HW_ASSISTED_COHERENCY`` is enabled, version 2 of
   translation library (xlat tables v2) must be used; version 1 of translation
   library is not supported.

-  ``INVERTED_MEMMAP``: memmap tool print by default lower addresses at the
   bottom, higher addresses at the top. This build flag can be set to '1' to
   invert this behavior. Lower addresses will be printed at the top and higher
   addresses at the bottom.

-  ``JUNO_AARCH32_EL3_RUNTIME``: This build flag enables you to execute EL3
   runtime software in AArch32 mode, which is required to run AArch32 on Juno.
   By default this flag is set to '0'. Enabling this flag builds BL1 and BL2 in
   AArch64 and facilitates the loading of ``SP_MIN`` and BL33 as AArch32 executable
   images.

-  ``KEY_ALG``: This build flag enables the user to select the algorithm to be
   used for generating the PKCS keys and subsequent signing of the certificate.
   It accepts 3 values: ``rsa``, ``rsa_1_5`` and ``ecdsa``. The option
   ``rsa_1_5`` is the legacy PKCS#1 RSA 1.5 algorithm which is not TBBR
   compliant and is retained only for compatibility. The default value of this
   flag is ``rsa`` which is the TBBR compliant PKCS#1 RSA 2.1 scheme.

-  ``KEY_SIZE``: This build flag enables the user to select the key size for
   the algorithm specified by ``KEY_ALG``. The valid values for ``KEY_SIZE``
   depend on the chosen algorithm and the cryptographic module.

   +-----------+------------------------------------+
   |  KEY_ALG  |        Possible key sizes          |
   +===========+====================================+
   |    rsa    | 1024 , 2048 (default), 3072, 4096* |
   +-----------+------------------------------------+
   |   ecdsa   |            unavailable             |
   +-----------+------------------------------------+

   * Only 2048 bits size is available with CryptoCell 712 SBROM release 1.
     Only 3072 bits size is available with CryptoCell 712 SBROM release 2.

-  ``HASH_ALG``: This build flag enables the user to select the secure hash
   algorithm. It accepts 3 values: ``sha256``, ``sha384`` and ``sha512``.
   The default value of this flag is ``sha256``.

-  ``LDFLAGS``: Extra user options appended to the linkers' command line in
   addition to the one set by the build system.

-  ``LOG_LEVEL``: Chooses the log level, which controls the amount of console log
   output compiled into the build. This should be one of the following:

   ::

       0  (LOG_LEVEL_NONE)
       10 (LOG_LEVEL_ERROR)
       20 (LOG_LEVEL_NOTICE)
       30 (LOG_LEVEL_WARNING)
       40 (LOG_LEVEL_INFO)
       50 (LOG_LEVEL_VERBOSE)

   All log output up to and including the selected log level is compiled into
   the build. The default value is 40 in debug builds and 20 in release builds.

-  ``MEASURED_BOOT``: Boolean flag to include support for the Measured Boot
   feature. If this flag is enabled ``TRUSTED_BOARD_BOOT`` must be set as well
   in order to provide trust that the code taking the measurements and recording
   them has not been tampered with.

   This option defaults to 0 and is an experimental feature in the stage of
   development.

-  ``NON_TRUSTED_WORLD_KEY``: This option is used when ``GENERATE_COT=1``. It
   specifies the file that contains the Non-Trusted World private key in PEM
   format. If ``SAVE_KEYS=1``, this file name will be used to save the key.

-  ``NS_BL2U``: Path to NS_BL2U image in the host file system. This image is
   optional. It is only needed if the platform makefile specifies that it
   is required in order to build the ``fwu_fip`` target.

-  ``NS_TIMER_SWITCH``: Enable save and restore for non-secure timer register
   contents upon world switch. It can take either 0 (don't save and restore) or
   1 (do save and restore). 0 is the default. An SPD may set this to 1 if it
   wants the timer registers to be saved and restored.

-  ``OVERRIDE_LIBC``: This option allows platforms to override the default libc
   for the BL image. It can be either 0 (include) or 1 (remove). The default
   value is 0.

-  ``PL011_GENERIC_UART``: Boolean option to indicate the PL011 driver that
   the underlying hardware is not a full PL011 UART but a minimally compliant
   generic UART, which is a subset of the PL011. The driver will not access
   any register that is not part of the SBSA generic UART specification.
   Default value is 0 (a full PL011 compliant UART is present).

-  ``PLAT``: Choose a platform to build TF-A for. The chosen platform name
   must be subdirectory of any depth under ``plat/``, and must contain a
   platform makefile named ``platform.mk``. For example, to build TF-A for the
   Arm Juno board, select PLAT=juno.

-  ``PRELOADED_BL33_BASE``: This option enables booting a preloaded BL33 image
   instead of the normal boot flow. When defined, it must specify the entry
   point address for the preloaded BL33 image. This option is incompatible with
   ``EL3_PAYLOAD_BASE``. If both are defined, ``EL3_PAYLOAD_BASE`` has priority
   over ``PRELOADED_BL33_BASE``.

-  ``PROGRAMMABLE_RESET_ADDRESS``: This option indicates whether the reset
   vector address can be programmed or is fixed on the platform. It can take
   either 0 (fixed) or 1 (programmable). Default is 0. If the platform has a
   programmable reset address, it is expected that a CPU will start executing
   code directly at the right address, both on a cold and warm reset. In this
   case, there is no need to identify the entrypoint on boot and the boot path
   can be optimised. The ``plat_get_my_entrypoint()`` platform porting interface
   does not need to be implemented in this case.

-  ``PSCI_EXTENDED_STATE_ID``: As per PSCI1.0 Specification, there are 2 formats
   possible for the PSCI power-state parameter: original and extended State-ID
   formats. This flag if set to 1, configures the generic PSCI layer to use the
   extended format. The default value of this flag is 0, which means by default
   the original power-state format is used by the PSCI implementation. This flag
   should be specified by the platform makefile and it governs the return value
   of PSCI_FEATURES API for CPU_SUSPEND smc function id. When this option is
   enabled on Arm platforms, the option ``ARM_RECOM_STATE_ID_ENC`` needs to be
   set to 1 as well.

-  ``RAS_EXTENSION``: When set to ``1``, enable Armv8.2 RAS features. RAS features
   are an optional extension for pre-Armv8.2 CPUs, but are mandatory for Armv8.2
   or later CPUs.

   When ``RAS_EXTENSION`` is set to ``1``, ``HANDLE_EA_EL3_FIRST`` must also be
   set to ``1``.

   This option is disabled by default.

-  ``RESET_TO_BL31``: Enable BL31 entrypoint as the CPU reset vector instead
   of the BL1 entrypoint. It can take the value 0 (CPU reset to BL1
   entrypoint) or 1 (CPU reset to BL31 entrypoint).
   The default value is 0.

-  ``RESET_TO_SP_MIN``: SP_MIN is the minimal AArch32 Secure Payload provided
   in TF-A. This flag configures SP_MIN entrypoint as the CPU reset vector
   instead of the BL1 entrypoint. It can take the value 0 (CPU reset to BL1
   entrypoint) or 1 (CPU reset to SP_MIN entrypoint). The default value is 0.

-  ``ROT_KEY``: This option is used when ``GENERATE_COT=1``. It specifies the
   file that contains the ROT private key in PEM format and enforces public key
   hash generation. If ``SAVE_KEYS=1``, this
   file name will be used to save the key.

-  ``SAVE_KEYS``: This option is used when ``GENERATE_COT=1``. It tells the
   certificate generation tool to save the keys used to establish the Chain of
   Trust. Allowed options are '0' or '1'. Default is '0' (do not save).

-  ``SCP_BL2``: Path to SCP_BL2 image in the host file system. This image is optional.
   If a SCP_BL2 image is present then this option must be passed for the ``fip``
   target.

-  ``SCP_BL2_KEY``: This option is used when ``GENERATE_COT=1``. It specifies the
   file that contains the SCP_BL2 private key in PEM format. If ``SAVE_KEYS=1``,
   this file name will be used to save the key.

-  ``SCP_BL2U``: Path to SCP_BL2U image in the host file system. This image is
   optional. It is only needed if the platform makefile specifies that it
   is required in order to build the ``fwu_fip`` target.

-  ``SDEI_SUPPORT``: Setting this to ``1`` enables support for Software
   Delegated Exception Interface to BL31 image. This defaults to ``0``.

   When set to ``1``, the build option ``EL3_EXCEPTION_HANDLING`` must also be
   set to ``1``.

-  ``SEPARATE_CODE_AND_RODATA``: Whether code and read-only data should be
   isolated on separate memory pages. This is a trade-off between security and
   memory usage. See "Isolating code and read-only data on separate memory
   pages" section in :ref:`Firmware Design`. This flag is disabled by default
   and affects all BL images.

-  ``SEPARATE_NOBITS_REGION``: Setting this option to ``1`` allows the NOBITS
   sections of BL31 (.bss, stacks, page tables, and coherent memory) to be
   allocated in RAM discontiguous from the loaded firmware image. When set, the
   platform is expected to provide definitions for ``BL31_NOBITS_BASE`` and
   ``BL31_NOBITS_LIMIT``. When the option is ``0`` (the default), NOBITS
   sections are placed in RAM immediately following the loaded firmware image.

-  ``SMC_PCI_SUPPORT``: This option allows platforms to handle PCI configuration
   access requests via a standard SMCCC defined in `DEN0115`_. When combined with
   UEFI+ACPI this can provide a certain amount of OS forward compatibility
   with newer platforms that aren't ECAM compliant.

-  ``SPD``: Choose a Secure Payload Dispatcher component to be built into TF-A.
   This build option is only valid if ``ARCH=aarch64``. The value should be
   the path to the directory containing the SPD source, relative to
   ``services/spd/``; the directory is expected to contain a makefile called
   ``<spd-value>.mk``. The SPM Dispatcher standard service is located in
   services/std_svc/spmd and enabled by ``SPD=spmd``. The SPM Dispatcher
   cannot be enabled when the ``SPM_MM`` option is enabled.

-  ``SPIN_ON_BL1_EXIT``: This option introduces an infinite loop in BL1. It can
   take either 0 (no loop) or 1 (add a loop). 0 is the default. This loop stops
   execution in BL1 just before handing over to BL31. At this point, all
   firmware images have been loaded in memory, and the MMU and caches are
   turned off. Refer to the "Debugging options" section for more details.

-  ``SPMD_SPM_AT_SEL2`` : this boolean option is used jointly with the SPM
   Dispatcher option (``SPD=spmd``). When enabled (1) it indicates the SPMC
   component runs at the S-EL2 execution state provided by the Armv8.4-SecEL2
   extension. This is the default when enabling the SPM Dispatcher. When
   disabled (0) it indicates the SPMC component runs at the S-EL1 execution
   state. This latter configuration supports pre-Armv8.4 platforms (aka not
   implementing the Armv8.4-SecEL2 extension).

-  ``SPM_MM`` : Boolean option to enable the Management Mode (MM)-based Secure
   Partition Manager (SPM) implementation. The default value is ``0``
   (disabled). This option cannot be enabled (``1``) when SPM Dispatcher is
   enabled (``SPD=spmd``).

-  ``SP_LAYOUT_FILE``: Platform provided path to JSON file containing the
   description of secure partitions. The build system will parse this file and
   package all secure partition blobs into the FIP. This file is not
   necessarily part of TF-A tree. Only available when ``SPD=spmd``.

-  ``SP_MIN_WITH_SECURE_FIQ``: Boolean flag to indicate the SP_MIN handles
   secure interrupts (caught through the FIQ line). Platforms can enable
   this directive if they need to handle such interruption. When enabled,
   the FIQ are handled in monitor mode and non secure world is not allowed
   to mask these events. Platforms that enable FIQ handling in SP_MIN shall
   implement the api ``sp_min_plat_fiq_handler()``. The default value is 0.

-  ``TRUSTED_BOARD_BOOT``: Boolean flag to include support for the Trusted Board
   Boot feature. When set to '1', BL1 and BL2 images include support to load
   and verify the certificates and images in a FIP, and BL1 includes support
   for the Firmware Update. The default value is '0'. Generation and inclusion
   of certificates in the FIP and FWU_FIP depends upon the value of the
   ``GENERATE_COT`` option.

   .. warning::
      This option depends on ``CREATE_KEYS`` to be enabled. If the keys
      already exist in disk, they will be overwritten without further notice.

-  ``TRUSTED_WORLD_KEY``: This option is used when ``GENERATE_COT=1``. It
   specifies the file that contains the Trusted World private key in PEM
   format. If ``SAVE_KEYS=1``, this file name will be used to save the key.

-  ``TSP_INIT_ASYNC``: Choose BL32 initialization method as asynchronous or
   synchronous, (see "Initializing a BL32 Image" section in
   :ref:`Firmware Design`). It can take the value 0 (BL32 is initialized using
   synchronous method) or 1 (BL32 is initialized using asynchronous method).
   Default is 0.

-  ``TSP_NS_INTR_ASYNC_PREEMPT``: A non zero value enables the interrupt
   routing model which routes non-secure interrupts asynchronously from TSP
   to EL3 causing immediate preemption of TSP. The EL3 is responsible
   for saving and restoring the TSP context in this routing model. The
   default routing model (when the value is 0) is to route non-secure
   interrupts to TSP allowing it to save its context and hand over
   synchronously to EL3 via an SMC.

   .. note::
      When ``EL3_EXCEPTION_HANDLING`` is ``1``, ``TSP_NS_INTR_ASYNC_PREEMPT``
      must also be set to ``1``.

-  ``USE_ARM_LINK``: This flag determines whether to enable support for ARM
   linker. When the ``LINKER`` build variable points to the armlink linker,
   this flag is enabled automatically. To enable support for armlink, platforms
   will have to provide a scatter file for the BL image. Currently, Tegra
   platforms use the armlink support to compile BL3-1 images.

-  ``USE_COHERENT_MEM``: This flag determines whether to include the coherent
   memory region in the BL memory map or not (see "Use of Coherent memory in
   TF-A" section in :ref:`Firmware Design`). It can take the value 1
   (Coherent memory region is included) or 0 (Coherent memory region is
   excluded). Default is 1.

-  ``USE_DEBUGFS``: When set to 1 this option activates an EXPERIMENTAL feature
   exposing a virtual filesystem interface through BL31 as a SiP SMC function.
   Default is 0.

-  ``ARM_IO_IN_DTB``: This flag determines whether to use IO based on the
   firmware configuration framework. This will move the io_policies into a
   configuration device tree, instead of static structure in the code base.
   This is currently an experimental feature.

-  ``COT_DESC_IN_DTB``: This flag determines whether to create COT descriptors
   at runtime using fconf. If this flag is enabled, COT descriptors are
   statically captured in tb_fw_config file in the form of device tree nodes
   and properties. Currently, COT descriptors used by BL2 are moved to the
   device tree and COT descriptors used by BL1 are retained in the code
   base statically. This is currently an experimental feature.

-  ``SDEI_IN_FCONF``: This flag determines whether to configure SDEI setup in
   runtime using firmware configuration framework. The platform specific SDEI
   shared and private events configuration is retrieved from device tree rather
   than static C structures at compile time. This is currently an experimental
   feature and is only supported if SDEI_SUPPORT build flag is enabled.

-  ``SEC_INT_DESC_IN_FCONF``: This flag determines whether to configure Group 0
   and Group1 secure interrupts using the firmware configuration framework. The
   platform specific secure interrupt property descriptor is retrieved from
   device tree in runtime rather than depending on static C structure at compile
   time. This is currently an experimental feature.

-  ``USE_ROMLIB``: This flag determines whether library at ROM will be used.
   This feature creates a library of functions to be placed in ROM and thus
   reduces SRAM usage. Refer to :ref:`Library at ROM` for further details. Default
   is 0.

-  ``V``: Verbose build. If assigned anything other than 0, the build commands
   are printed. Default is 0.

-  ``VERSION_STRING``: String used in the log output for each TF-A image.
   Defaults to a string formed by concatenating the version number, build type
   and build string.

-  ``W``: Warning level. Some compiler warning options of interest have been
   regrouped and put in the root Makefile. This flag can take the values 0 to 3,
   each level enabling more warning options. Default is 0.

-  ``WARMBOOT_ENABLE_DCACHE_EARLY`` : Boolean option to enable D-cache early on
   the CPU after warm boot. This is applicable for platforms which do not
   require interconnect programming to enable cache coherency (eg: single
   cluster platforms). If this option is enabled, then warm boot path
   enables D-caches immediately after enabling MMU. This option defaults to 0.

-  ``SUPPORT_STACK_MEMTAG``: This flag determines whether to enable memory
   tagging for stack or not. It accepts 2 values: ``yes`` and ``no``. The
   default value of this flag is ``no``. Note this option must be enabled only
   for ARM architecture greater than Armv8.5-A.

-  ``ERRATA_SPECULATIVE_AT``: This flag determines whether to enable ``AT``
   speculative errata workaround or not. It accepts 2 values: ``1`` and ``0``.
   The default value of this flag is ``0``.

   ``AT`` speculative errata workaround disables stage1 page table walk for
   lower ELs (EL1 and EL0) in EL3 so that ``AT`` speculative fetch at any point
   produces either the correct result or failure without TLB allocation.

   This boolean option enables errata for all below CPUs.

   +---------+--------------+-------------------------+
   | Errata  |      CPU     |     Workaround Define   |
   +=========+==============+=========================+
   | 1165522 |  Cortex-A76  |  ``ERRATA_A76_1165522`` |
   +---------+--------------+-------------------------+
   | 1319367 |  Cortex-A72  |  ``ERRATA_A72_1319367`` |
   +---------+--------------+-------------------------+
   | 1319537 |  Cortex-A57  |  ``ERRATA_A57_1319537`` |
   +---------+--------------+-------------------------+
   | 1530923 |  Cortex-A55  |  ``ERRATA_A55_1530923`` |
   +---------+--------------+-------------------------+
   | 1530924 |  Cortex-A53  |  ``ERRATA_A53_1530924`` |
   +---------+--------------+-------------------------+

   .. note::
      This option is enabled by build only if platform sets any of above defines
      mentioned in ’Workaround Define' column in the table.
      If this option is enabled for the EL3 software then EL2 software also must
      implement this workaround due to the behaviour of the errata mentioned
      in new SDEN document which will get published soon.

- ``RAS_TRAP_LOWER_EL_ERR_ACCESS``: This flag enables/disables the SCR_EL3.TERR
  bit, to trap access to the RAS ERR and RAS ERX registers from lower ELs.
  This flag is disabled by default.

- ``OPENSSL_DIR``: This flag is used to provide the installed openssl directory
  path on the host machine which is used to build certificate generation and
  firmware encryption tool.

- ``USE_SP804_TIMER``: Use the SP804 timer instead of the Generic Timer for
  functions that wait for an arbitrary time length (udelay and mdelay). The
  default value is 0.

GICv3 driver options
--------------------

GICv3 driver files are included using directive:

``include drivers/arm/gic/v3/gicv3.mk``

The driver can be configured with the following options set in the platform
makefile:

-  ``GICV3_SUPPORT_GIC600``: Add support for the GIC-600 variants of GICv3.
   Enabling this option will add runtime detection support for the
   GIC-600, so is safe to select even for a GIC500 implementation.
   This option defaults to 0.

-  ``GICV3_IMPL_GIC600_MULTICHIP``: Selects GIC-600 variant with multichip
   functionality. This option defaults to 0

-  ``GICV3_OVERRIDE_DISTIF_PWR_OPS``: Allows override of default implementation
   of ``arm_gicv3_distif_pre_save`` and ``arm_gicv3_distif_post_restore``
   functions. This is required for FVP platform which need to simulate GIC save
   and restore during SYSTEM_SUSPEND without powering down GIC. Default is 0.

-  ``GIC_ENABLE_V4_EXTN`` : Enables GICv4 related changes in GICv3 driver.
   This option defaults to 0.

-  ``GIC_EXT_INTID``: When set to ``1``, GICv3 driver will support extended
   PPI (1056-1119) and SPI (4096-5119) range. This option defaults to 0.

Debugging options
-----------------

To compile a debug version and make the build more verbose use

.. code:: shell

    make PLAT=<platform> DEBUG=1 V=1 all

AArch64 GCC uses DWARF version 4 debugging symbols by default. Some tools (for
example DS-5) might not support this and may need an older version of DWARF
symbols to be emitted by GCC. This can be achieved by using the
``-gdwarf-<version>`` flag, with the version being set to 2 or 3. Setting the
version to 2 is recommended for DS-5 versions older than 5.16.

When debugging logic problems it might also be useful to disable all compiler
optimizations by using ``-O0``.

.. warning::
   Using ``-O0`` could cause output images to be larger and base addresses
   might need to be recalculated (see the **Memory layout on Arm development
   platforms** section in the :ref:`Firmware Design`).

Extra debug options can be passed to the build system by setting ``CFLAGS`` or
``LDFLAGS``:

.. code:: shell

    CFLAGS='-O0 -gdwarf-2'                                     \
    make PLAT=<platform> DEBUG=1 V=1 all

Note that using ``-Wl,`` style compilation driver options in ``CFLAGS`` will be
ignored as the linker is called directly.

It is also possible to introduce an infinite loop to help in debugging the
post-BL2 phase of TF-A. This can be done by rebuilding BL1 with the
``SPIN_ON_BL1_EXIT=1`` build flag. Refer to the :ref:`build_options_common`
section. In this case, the developer may take control of the target using a
debugger when indicated by the console output. When using DS-5, the following
commands can be used:

::

    # Stop target execution
    interrupt

    #
    # Prepare your debugging environment, e.g. set breakpoints
    #

    # Jump over the debug loop
    set var $AARCH64::$Core::$PC = $AARCH64::$Core::$PC + 4

    # Resume execution
    continue

--------------

*Copyright (c) 2019-2021, Arm Limited. All rights reserved.*

.. _DEN0115: https://developer.arm.com/docs/den0115/latest

