/*
 * Copyright (c) 2018, ARM Limited and Contributors. All rights reserved.
 *
 * SPDX-License-Identifier: BSD-3-Clause
 */

/dts-v1/;

/ {
	/* Platform Config */
	plat_arm_bl2 {
		compatible = "arm,tb_fw";
		hw_config_addr = <0x0 0x82000000>;
		hw_config_max_size = <0x01000000>;
		/* Disable authentication for development */
		disable_auth = <0x0>;
		/*
		 * Load SoC and TOS firmware configs at the base of
		 * non shared SRAM. The runtime checks ensure we don't
		 * overlap BL2, BL31 or BL32. The NT firmware config
		 * is loaded at base of DRAM.
		 */
		soc_fw_config_addr = <0x0 0x04001000>;
		soc_fw_config_max_size = <0x200>;
		tos_fw_config_addr = <0x0 0x04001200>;
		tos_fw_config_max_size = <0x200>;
		nt_fw_config_addr = <0x0 0x80000000>;
		nt_fw_config_max_size = <0x200>;
	};
};
