/*
 * Copyright (c) 2020, Arm Limited. All rights reserved.
 *
 * SPDX-License-Identifier: BSD-3-Clause
 */

/dts-v1/;

/ {
	compatible = "arm,tc0";
	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	aliases {
		serial0 = &soc_uart0;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu-map {
			cluster0 {
				core0 {
					cpu = <&CPU0>;
				};
				core1 {
					cpu = <&CPU1>;
				};
				core2 {
					cpu = <&CPU2>;
				};
				core3 {
					cpu = <&CPU3>;
				};
				core4 {
					cpu = <&CPU4>;
				};
				core5 {
					cpu = <&CPU5>;
				};
				core6 {
					cpu = <&CPU6>;
				};
				core7 {
					cpu = <&CPU7>;
				};
			};
		};

		/*
		 * The timings below are just to demonstrate working cpuidle.
		 * These values may be inaccurate.
		 */
		idle-states {
			entry-method = "arm,psci";

			CPU_SLEEP_0: cpu-sleep-0 {
				compatible = "arm,idle-state";
				arm,psci-suspend-param = <0x0010000>;
				local-timer-stop;
				entry-latency-us = <300>;
				exit-latency-us = <1200>;
				min-residency-us = <2000>;
			};
			CLUSTER_SLEEP_0: cluster-sleep-0 {
				compatible = "arm,idle-state";
				arm,psci-suspend-param = <0x1010000>;
				local-timer-stop;
				entry-latency-us = <400>;
				exit-latency-us = <1200>;
				min-residency-us = <2500>;
			};
		};

		CPU0:cpu@0 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x0>;
			enable-method = "psci";
			clocks = <&scmi_dvfs 0>;
			cpu-idle-states = <&CPU_SLEEP_0 &CLUSTER_SLEEP_0>;
		};

		CPU1:cpu@100 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x100>;
			enable-method = "psci";
			clocks = <&scmi_dvfs 0>;
			cpu-idle-states = <&CPU_SLEEP_0 &CLUSTER_SLEEP_0>;
		};

		CPU2:cpu@200 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x200>;
			enable-method = "psci";
			clocks = <&scmi_dvfs 0>;
			cpu-idle-states = <&CPU_SLEEP_0 &CLUSTER_SLEEP_0>;
		};

		CPU3:cpu@300 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x300>;
			enable-method = "psci";
			clocks = <&scmi_dvfs 0>;
			cpu-idle-states = <&CPU_SLEEP_0 &CLUSTER_SLEEP_0>;
		};

		CPU4:cpu@400 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x400>;
			enable-method = "psci";
			clocks = <&scmi_dvfs 1>;
			cpu-idle-states = <&CPU_SLEEP_0 &CLUSTER_SLEEP_0>;
		};

		CPU5:cpu@500 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x500>;
			enable-method = "psci";
			clocks = <&scmi_dvfs 1>;
			cpu-idle-states = <&CPU_SLEEP_0 &CLUSTER_SLEEP_0>;
		};

		CPU6:cpu@600 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x600>;
			enable-method = "psci";
			clocks = <&scmi_dvfs 1>;
			cpu-idle-states = <&CPU_SLEEP_0 &CLUSTER_SLEEP_0>;
		};

		CPU7:cpu@700 {
			device_type = "cpu";
			compatible = "arm,armv8";
			reg = <0x700>;
			enable-method = "psci";
			clocks = <&scmi_dvfs 1>;
			cpu-idle-states = <&CPU_SLEEP_0 &CLUSTER_SLEEP_0>;
		};

	};

	memory@80000000 {
		device_type = "memory";
		reg = <0x0 0x80000000 0x0 0x7d000000>;
	};

	reserved-memory {
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		optee@0xfce00000 {
			reg = <0x00000000 0xfce00000 0 0x00200000>;
			no-map;
		};
	};

	psci {
		compatible = "arm,psci-1.0", "arm,psci-0.2", "arm,psci";
		method = "smc";
	};

	sram: sram@6000000 {
		compatible = "mmio-sram";
		reg = <0x0 0x06000000 0x0 0x8000>;

		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0 0x0 0x06000000 0x8000>;

		cpu_scp_scmi_mem: scp-shmem@0 {
			compatible = "arm,scmi-shmem";
			reg = <0x0 0x80>;
		};
	};

	mbox_db_rx: mhu@45010000 {
		compatible = "arm,mhuv2","arm,primecell";
		reg = <0x0 0x45010000 0x0 0x1000>;
		clocks = <&soc_refclk100mhz>;
		clock-names = "apb_pclk";
		#mbox-cells = <1>;
		interrupts = <0 317 4>;
		interrupt-names = "mhu_rx";
		mhu-protocol = "doorbell";
	};

	mbox_db_tx: mhu@45000000 {
		compatible = "arm,mhuv2","arm,primecell";
		reg = <0x0 0x45000000 0x0 0x1000>;
		clocks = <&soc_refclk100mhz>;
		clock-names = "apb_pclk";
		#mbox-cells = <1>;
		interrupt-names = "mhu_tx";
		mhu-protocol = "doorbell";
	};

	scmi {
		compatible = "arm,scmi";
		method = "mailbox-doorbell";
		mbox-names = "tx", "rx";
		mboxes = <&mbox_db_tx 0 &mbox_db_rx 0>;
		shmem = <&cpu_scp_scmi_mem &cpu_scp_scmi_mem>;
		#address-cells = <1>;
		#size-cells = <0>;

		scmi_dvfs: protocol@13 {
			reg = <0x13>;
			#clock-cells = <1>;
		};

		scmi_clk: protocol@14 {
			reg = <0x14>;
			#clock-cells = <1>;
		};
	};

	gic: interrupt-controller@2c010000 {
		compatible = "arm,gic-600", "arm,gic-v3";
		#address-cells = <2>;
		#interrupt-cells = <3>;
		#size-cells = <2>;
		ranges;
		interrupt-controller;
		reg = <0x0 0x30000000 0 0x10000>, /* GICD */
		      <0x0 0x30140000 0 0x200000>; /* GICR */
		interrupts = <0x1 0x9 0x4>;
	};

	timer {
		compatible = "arm,armv8-timer";
		interrupts = <0x1 13 0x8>,
			     <0x1 14 0x8>,
			     <0x1 11 0x8>,
			     <0x1 10 0x8>;
	};

	soc_refclk100mhz: refclk100mhz {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <100000000>;
		clock-output-names = "apb_pclk";
	};

	soc_refclk60mhz: refclk60mhz {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <60000000>;
		clock-output-names = "iofpga_clk";
	};

	soc_uartclk:  uartclk {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <50000000>;
		clock-output-names = "uartclk";
	};

	soc_uart0: uart@7ff80000 {
		compatible = "arm,pl011", "arm,primecell";
		reg = <0x0 0x7ff80000 0x0 0x1000>;
		interrupts = <0x0 116 0x4>;
		clocks = <&soc_uartclk>, <&soc_refclk100mhz>;
		clock-names = "uartclk", "apb_pclk";
		status = "okay";
	};

	vencoder {
		compatible = "drm,virtual-encoder";

		port {
			vencoder_in: endpoint {
				remote-endpoint = <&dp_pl0_out0>;
			};
		};

		display-timings {
			panel-timing {
				clock-frequency = <25175000>;
				hactive = <640>;
				vactive = <480>;
				hfront-porch = <16>;
				hback-porch = <48>;
				hsync-len = <96>;
				vfront-porch = <10>;
				vback-porch = <33>;
				vsync-len = <2>;
			};
		};

	};

	hdlcd: hdlcd@7ff60000 {
		compatible = "arm,hdlcd";
		reg = <0x0 0x7ff60000 0x0 0x1000>;
		interrupts = <0x0 117 0x4>;
		clocks = <&fake_hdlcd_clk>;
		clock-names = "pxlclk";
		status = "disabled";

		port {
			hdlcd_out: endpoint {
				remote-endpoint = <&vencoder_in>;
			};
		};
	};

	fake_hdlcd_clk: fake-hdlcd-clk {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <25175000>;
		clock-output-names = "pxlclk";
	};

	ethernet@18000000 {
		compatible = "smsc,lan91c111";
		reg = <0x0 0x18000000 0x0 0x10000>;
		interrupts = <0 109 4>;
	};

	kmi@1c060000 {
		compatible = "arm,pl050", "arm,primecell";
		reg = <0x0 0x001c060000 0x0 0x1000>;
		interrupts = <0 197 4>;
		clocks = <&bp_clock24mhz>, <&bp_clock24mhz>;
		clock-names = "KMIREFCLK", "apb_pclk";
	};

	kmi@1c070000 {
		compatible = "arm,pl050", "arm,primecell";
		reg = <0x0 0x001c070000 0x0 0x1000>;
		interrupts = <0 103 4>;
		clocks = <&bp_clock24mhz>, <&bp_clock24mhz>;
		clock-names = "KMIREFCLK", "apb_pclk";
	};

	bp_clock24mhz: clock24mhz {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <24000000>;
		clock-output-names = "bp:clock24mhz";
	};

	virtio_block@1c130000 {
		compatible = "virtio,mmio";
		reg = <0x0 0x1c130000 0x0 0x200>;
		interrupts = <0 204 4>;
	};

	sysreg: sysreg@1c010000 {
		compatible = "arm,vexpress-sysreg";
		reg = <0x0 0x001c010000 0x0 0x1000>;
		gpio-controller;
		#gpio-cells = <2>;
	};

	fixed_3v3: v2m-3v3 {
		compatible = "regulator-fixed";
		regulator-name = "3V3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
	};

	mmci@1c050000 {
		compatible = "arm,pl180", "arm,primecell";
		reg = <0x0 0x001c050000 0x0 0x1000>;
		interrupts = <0 107 0x4>,
			     <0 108 0x4>;
		cd-gpios = <&sysreg 0 0>;
		wp-gpios = <&sysreg 1 0>;
		bus-width = <8>;
		max-frequency = <12000000>;
		vmmc-supply = <&fixed_3v3>;
		clocks = <&bp_clock24mhz>, <&bp_clock24mhz>;
		clock-names = "mclk", "apb_pclk";
	};

	dp0: display@2cc00000 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "arm,mali-d71";
		reg = <0 0x2cc00000 0 0x20000>;
		interrupts = <0 69 4>;
		interrupt-names = "DPU";
		clocks = <&scmi_clk 0>;
		clock-names = "aclk";
		pl0: pipeline@0 {
			reg = <0>;
			clocks = <&scmi_clk 1>;
			clock-names = "pxclk";
			pl_id = <0>;
			ports {
				#address-cells = <1>;
				#size-cells = <0>;
				port@0 {
					reg = <0>;
					dp_pl0_out0: endpoint {
						remote-endpoint = <&vencoder_in>;
					};
				};
			};
		};

		pl1: pipeline@1 {
			reg = <1>;
			clocks = <&scmi_clk 2>;
			clock-names = "pxclk";
			pl_id = <1>;
			ports {
				#address-cells = <1>;
				#size-cells = <0>;
				port@0 {
					reg = <0>;
				};
			};
		};
	};

	ffa {
		compatible = "arm,ffa";
		conduit = "smc";
		mem_share_buffer = "tx";
	};

	firmware {
		optee {
		      compatible = "linaro,optee-tz";
		      method = "ffa";
		};
	};
};
