/*
 * Copyright (c) 2019-2020, Arm Limited. All rights reserved.
 *
 * SPDX-License-Identifier: BSD-3-Clause
 */

/dts-v1/;

/ {
	model = "V2F-1XV7 Cortex-A7x1 SMM";
	compatible = "arm,vexpress,v2f-1xv7", "arm,vexpress";
	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	cpus {
		#address-cells = <2>;
		#size-cells = <0>;

		cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a7";
			reg = <0 0>;
		};
	};

	memory@0,80000000 {
		device_type = "memory";
		reg = <0 0x80000000 0 0x80000000>; /* 2GB @ 2GB */
	};

	gic: interrupt-controller@2c001000 {
		compatible = "arm,cortex-a15-gic";
		#interrupt-cells = <3>;
		#address-cells = <0>;
		interrupt-controller;
		reg = <0 0x2c001000 0 0x1000>,
		      <0 0x2c002000 0 0x1000>,
		      <0 0x2c004000 0 0x2000>,
		      <0 0x2c006000 0 0x2000>;
		interrupts = <1 9 0xf04>;
	};

	smbclk: refclk24mhzx2 {
		/* Reference 24MHz clock x 2 */
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <48000000>;
		clock-output-names = "smclk";
	};

	smb {
		compatible = "simple-bus";

		#address-cells = <2>;
		#size-cells = <1>;
		ranges = <0 0 0 0x08000000 0x04000000>,
			 <1 0 0 0x14000000 0x04000000>,
			 <2 0 0 0x18000000 0x04000000>,
			 <3 0 0 0x1c000000 0x04000000>,
			 <4 0 0 0x0c000000 0x04000000>,
			 <5 0 0 0x10000000 0x04000000>;

		#interrupt-cells = <1>;
		interrupt-map-mask = <0 0 63>;
		interrupt-map = <0 0  0 &gic 0  0 4>,
				<0 0  1 &gic 0  1 4>,
				<0 0  2 &gic 0  2 4>,
				<0 0  3 &gic 0  3 4>,
				<0 0  4 &gic 0  4 4>,
				<0 0  5 &gic 0  5 4>,
				<0 0 42 &gic 0 42 4>;

		#include "rtsm_ve-motherboard-aarch32.dtsi"
	};
};
