Description
===========

MediaTek 8183 (MT8183) is a 64-bit ARM SoC introduced by MediaTek in early 2018.
The chip incorporates eight cores - four Cortex-A53 little cores and Cortex-A73.
Both clusters can operate at up to 2 GHz.

Boot Sequence
=============

::

    Boot Rom --> Coreboot --> TF-A BL31 --> Depthcharge --> Linux Kernel

How to Build
============

.. code:: shell

    make CROSS_COMPILE=aarch64-linux-gnu- PLAT=mt8183 DEBUG=1
